<map id="G" name="G">
<area shape="rect" id="node3" href="$group___m_i_o_s32___i_r_q.html#gaf120e75527ddf938d55b8504aaa44a44" title="MIOS32_IRQ_Disable" alt="" coords="440,5,581,35"/>
<area shape="rect" id="node5" href="$group___m_i_o_s32___i_r_q.html#ga277a766732d6882cad13a4d6c7e03d03" title="MIOS32_IRQ_Enable" alt="" coords="441,59,580,88"/>
<area shape="rect" id="node7" href="$group___m_i_o_s32___s_y_s.html#gae6c2655f023610e359a2e0d4ffed978e" title="MIOS32_SYS_SerialNumberGet" alt="" coords="127,616,324,645"/>
<area shape="rect" id="node9" href="$group___m_i_o_s32___u_s_b.html#ga04f4213b17b6b246497898d2fc964866" title="MIOS32_USB_Init" alt="" coords="165,405,285,435"/>
<area shape="rect" id="node43" href="$_l_p_c17xx_2msd_8c.html#a1086b3de30b66410609eb1ee7664d9c0" title="MSD_LUN_AvailableSet" alt="" coords="720,1029,877,1059"/>
<area shape="rect" id="node45" href="$msd__bot_8c.html#aa4fd3d58412644ba379861ee57f2ac1b" title="MSD_Mass_Storage_In" alt="" coords="435,851,587,880"/>
<area shape="rect" id="node80" href="$msd__bot_8c.html#ac6f5f16c479f87a380bd684403aa0472" title="MSD_Mass_Storage_Out" alt="" coords="145,1353,305,1383"/>
<area shape="rect" id="node13" href="$group___m_i_o_s32___i_r_q.html#gaee4f0cb19a6c739730cb63701ff9d038" title="MIOS32_IRQ_Install" alt="" coords="732,613,865,643"/>
<area shape="rect" id="node15" href="$group___m_i_o_s32___u_s_b___c_o_m.html#ga759ffee7cf728375766210128edd384b" title="MIOS32_USB_COM_ChangeConnectionState" alt="" coords="373,693,648,723"/>
<area shape="rect" id="node17" href="$group___m_i_o_s32___u_s_b___c_o_m.html#ga26257af1a693f2ee330b49da3d7f8bfd" title="MIOS32_USB_COM_EP3_OUT_Callback" alt="" coords="385,747,636,776"/>
<area shape="rect" id="node19" href="$group___m_i_o_s32___u_s_b___c_o_m.html#gae502932e4b2756882c1d459af63702ac" title="MIOS32_USB_COM_EP4_IN_Callback" alt="" coords="392,112,629,141"/>
<area shape="rect" id="node21" href="$group___m_i_o_s32___u_s_b.html#ga8809212e638558e939722df5c4a7ea83" title="MIOS32_USB_ForceDeviceMode" alt="" coords="408,165,613,195"/>
<area shape="rect" id="node23" href="$group___m_i_o_s32___u_s_b.html#ga1c45b294290f30c660cf21e515d660c8" title="MIOS32_USB_IsInitialized" alt="" coords="428,219,593,248"/>
<area shape="rect" id="node25" href="$group___m_i_o_s32___u_s_b___m_i_d_i.html#ga3e188912143937bc3a98d8d38863cb80" title="MIOS32_USB_MIDI_ChangeConnectionState" alt="" coords="375,272,647,301"/>
<area shape="rect" id="node27" href="$group___m_i_o_s32___u_s_b___m_i_d_i.html#gab0db37e589f56ca0585cbc3e8955abdb" title="MIOS32_USB_MIDI_EP1_IN_Callback" alt="" coords="393,325,628,355"/>
<area shape="rect" id="node29" href="$group___m_i_o_s32___u_s_b___m_i_d_i.html#ga57f933239657de8302082980eaf81f3e" title="MIOS32_USB_MIDI_EP2_OUT_Callback" alt="" coords="388,379,633,408"/>
<area shape="rect" id="node31" href="$group___m_i_o_s32___u_s_b.html#ga38bdd94d09d00f27d1343fdb0babdfa1" title="USB_OTG_BSP_EnableInterrupt Enabele USB Global interrupt." alt="" coords="411,640,611,669"/>
<area shape="rect" id="node34" href="$group___m_i_o_s32___u_s_b.html#gacffb89e4346b11dee704fe5a40326a1f" title="USB_OTG_BSP_Init Initilizes BSP configurations." alt="" coords="444,432,577,461"/>
<area shape="rect" id="node36" href="$group___m_i_o_s32___u_s_b.html#ga28c906bec05a1b7f91aa0e4ff5d8a16c" title="USB_OTG_BSP_mDelay This function provides delay time in milli sec." alt="" coords="432,536,589,565"/>
<area shape="rect" id="node38" href="$group___m_i_o_s32___u_s_b.html#gaa70213d9a7b9b047dc6d3357f99e19b5" title="USB_OTG_BSP_uDelay This function provides delay time in micro sec." alt="" coords="721,509,876,539"/>
<area shape="rect" id="node40" href="$group___m_i_o_s32___d_e_l_a_y.html#ga4a62f99a75fe22d9d02f1dd635432a27" title="MIOS32_DELAY_Wait_uS" alt="" coords="987,509,1152,539"/>
<area shape="rect" id="node47" href="$msd__scsi_8c.html#af170aa17db1c311ea568c8e80cdc3d5a" title="MSD_SCSI_Read10_Cmd" alt="" coords="715,1159,883,1188"/>
<area shape="rect" id="node73" href="$msd__bot_8c.html#a0dcaf7a0e985945e5b8e9f81fce31c74" title="MSD_Set_CSW" alt="" coords="1281,1264,1391,1293"/>
<area shape="rect" id="node49" href="$msd__bot_8c.html#a5679b525a29485f70d93496c8afc0570" title="MSD_Bot_Abort" alt="" coords="1281,1496,1391,1525"/>
<area shape="rect" id="node51" href="$msd__memory_8c.html#aa539545834e47e46beec981712dc30f2" title="MSD_Read_Memory" alt="" coords="1001,953,1137,983"/>
<area shape="rect" id="node70" href="$msd__scsi_8c.html#a4af417341472e50263529cac4e8e07bc" title="MSD_SCSI_Address_Management" alt="" coords="963,1212,1176,1241"/>
<area shape="rect" id="node75" href="$msd__scsi_8c.html#ad1e7d4eee0f2649f9c47035fec2b6e77" title="MSD_Set_Scsi_Sense_Data" alt="" coords="1247,1703,1425,1732"/>
<area shape="rect" id="node53" href="$group___m_i_o_s32___s_d_c_a_r_d.html#ga1f1d927bd75ab940e2613e94992fbc2a" title="MIOS32_SDCARD_SectorRead" alt="" coords="1237,953,1435,983"/>
<area shape="rect" id="node55" href="$group___m_i_o_s32___s_d_c_a_r_d.html#gaf9dae6d1c88d7b32241e4fbe87d0037c" title="MIOS32_SDCARD_SendSDCCmd" alt="" coords="1483,877,1696,907"/>
<area shape="rect" id="node58" href="$group___m_i_o_s32___s_p_i.html#gafa4ea61a948eab9ce0a778b6b010a5d4" title="MIOS32_SPI_RC_PinSet" alt="" coords="1748,877,1908,907"/>
<area shape="rect" id="node60" href="$group___m_i_o_s32___s_p_i.html#ga5d9702d52c2729bcfa132d497a5837a4" title="MIOS32_SPI_TransferByte" alt="" coords="1744,1032,1912,1061"/>
<area shape="rect" id="node63" href="$group___m_i_o_s32___s_p_i.html#gabcdae72100df8b893ee4684ad6763afb" title="MIOS32_SPI_TransferBlock" alt="" coords="1503,1085,1676,1115"/>
<area shape="rect" id="node67" href="$group___m_i_o_s32___s_p_i.html#ga97ec29423bee4eaf11f3d3bca206d9e1" title="MIOS32_SPI_TransferModeInit" alt="" coords="1495,1032,1684,1061"/>
<area shape="rect" id="node83" href="$msd__bot_8c.html#a921b762a044e31ee3b4580aa4f83e28e" title="MSD_CBW_Decode" alt="" coords="444,1676,577,1705"/>
<area shape="rect" id="node136" href="$msd__scsi_8c.html#a2ae335895be3ec41c6b16bca82bf6946" title="MSD_SCSI_Write10_Cmd" alt="" coords="716,1212,881,1241"/>
<area shape="rect" id="node87" href="$msd__scsi_8c.html#ae8a2376716ba9554a84f40e59c4f8005" title="MSD_SCSI_Format_Cmd" alt="" coords="988,1729,1151,1759"/>
<area shape="rect" id="node94" href="$msd__scsi_8c.html#a34d7ca38702a195cdc79930c4dd56bb6" title="MSD_SCSI_Inquiry_Cmd" alt="" coords="719,1935,879,1964"/>
<area shape="rect" id="node98" href="$msd__scsi_8c.html#a08dfb58a45d89b8afa5747efdad374d2" title="MSD_SCSI_ModeSense10_Cmd" alt="" coords="697,2145,900,2175"/>
<area shape="rect" id="node101" href="$msd__scsi_8c.html#ab23db213b76390e1fe27b834091b3e2f" title="MSD_SCSI_ModeSense6_Cmd" alt="" coords="700,2092,897,2121"/>
<area shape="rect" id="node105" href="$msd__scsi_8c.html#a95fb0d7d9caf68f02d4a31deda845d38" title="MSD_SCSI_ReadCapacity10_Cmd" alt="" coords="961,1887,1177,1916"/>
<area shape="rect" id="node112" href="$msd__scsi_8c.html#a5496995941e8c69b23ffe4b44d3ad8c6" title="MSD_SCSI_ReadFormatCapacity_Cmd" alt="" coords="949,1783,1189,1812"/>
<area shape="rect" id="node119" href="$msd__scsi_8c.html#a1944b893b594f9a86c17cde68bde6064" title="MSD_SCSI_RequestSense_Cmd" alt="" coords="696,1988,901,2017"/>
<area shape="rect" id="node122" href="$msd__scsi_8c.html#a30abf4d83ed9a74b49110e7e4a2af055" title="MSD_SCSI_Start_Stop_Unit_Cmd" alt="" coords="964,1316,1175,1345"/>
<area shape="rect" id="node125" href="$msd__scsi_8c.html#aed14586dc3f1ca4b828262b2fec7bc21" title="MSD_SCSI_TestUnitReady_Cmd" alt="" coords="967,1676,1172,1705"/>
<area shape="rect" id="node131" href="$msd__scsi_8c.html#aa5751aacbc04bc145bf63199f764bf21" title="MSD_SCSI_Verify10_Cmd" alt="" coords="985,1521,1153,1551"/>
<area shape="rect" id="node90" href="$msd__memory_8c.html#a0ba8031b6708d1ac42b5d44253ff72b5" title="MSD_MAL_GetStatus" alt="" coords="1265,1769,1407,1799"/>
<area shape="rect" id="node96" href="$msd__bot_8c.html#acb3bd0c0ff131fd724713aef9d3d0c82" title="MSD_Transfer_Data_Request" alt="" coords="1243,1964,1429,1993"/>
<area shape="rect" id="node142" href="$msd__memory_8c.html#ad3bccdf4d261868a7e93d1314448e086" title="MSD_Write_Memory" alt="" coords="1003,1007,1136,1036"/>
<area shape="rect" id="node144" href="$group___m_i_o_s32___s_d_c_a_r_d.html#ga317f2f51240b3c5770ab4ceba9db382f" title="MIOS32_SDCARD_SectorWrite" alt="" coords="1239,1019,1433,1048"/>
</map>
