# sysex_timeout_ctr_flags_t Union Reference
[MIOS32_MIDI]

## Data Fields
struct {
unsigned long long ALL
}; |
struct {
unsigned long long usb_receives:16
unsigned long long sysex_timeout_ctr_flags_t::iic_receives:16
unsigned long long sysex_timeout_ctr_flags_t::spi_receives:16
}; |

## Field Documentation

struct { ... }

unsigned long long sysex_timeout_ctr_flags_t::ALL

unsigned long long sysex_timeout_ctr_flags_t::usb_receives

The documentation for this union was generated from the following file:

- mios32/common/mios32_midi.c