# modules/msd/STM32F10x/msd_scsi_data.c File Reference

`#include "msd_scsi.h"`
`#include "msd_memory.h"`

## Variables
uint8_t | MSD_Page00_Inquiry_Data []
uint8_t | MSD_Standard_Inquiry_Data []
uint8_t | MSD_Standard_Inquiry_Data2 []
uint8_t | MSD_Mode_Sense6_data []
uint8_t | MSD_Mode_Sense10_data []
uint8_t | MSD_Scsi_Sense_Data []
uint8_t | MSD_ReadCapacity10_Data []
uint8_t | MSD_ReadFormatCapacity_Data []

## Variable Documentation

uint8_t MSD_Mode_Sense10_data[]

Initial value:

      {
        0x00,
        0x06,
        0x00,
        0x00,
        0x00,
        0x00,
        0x00,
        0x00
      }

uint8_t MSD_Mode_Sense6_data[]

Initial value:

      {
        0x03,
        0x00,
        0x00,
        0x00,
      }

uint8_t MSD_Page00_Inquiry_Data[]

Initial value:

      {
        0x00,
        0x00,
        0x00,
        0x00,
        0x00
      }

uint8_t MSD_ReadCapacity10_Data[]

Initial value:

      {

        0,
        0,
        0,
        0,

        0,
        0,
        0,
        0
      }

uint8_t MSD_ReadFormatCapacity_Data[]

Initial value:

      {
        0x00,
        0x00,
        0x00,
        0x08,

        0,
        0,
        0,
        0,

        0x02,
        0,
        0,
        0
      }

uint8_t MSD_Scsi_Sense_Data[]

Initial value:

      {
        0x70,
        0x00,
        NO_SENSE,
        0x00,
        0x00,
        0x00,
        0x00,
        0x0A,
        0x00,
        0x00,
        0x00,
        0x00,
        NO_SENSE,
        0x00,
        0x00,
        0x00,
        0x00,
        0x00
      }

uint8_t MSD_Standard_Inquiry_Data[]

Initial value:

      {
        0x00,
        0x80,
        0x02,
        0x02,

        36 - 4,
        0x00,
        0x00,
        0x00,

        'S', 'T', 'M', ' ', ' ', ' ', ' ', ' ',

        'S', 'D', ' ', 'F', 'l', 'a', 's', 'h', ' ',
        'D', 'i', 's', 'k', ' ', ' ', ' ',

        '1', '.', '0', ' '
      }

uint8_t MSD_Standard_Inquiry_Data2[]

Initial value:

      {
        0x00,
        0x80,
        0x02,
        0x02,

        36 - 4,
        0x00,
        0x00,
        0x00,

        'S', 'T', 'M', ' ', ' ', ' ', ' ', ' ',

        'N', 'A', 'N', 'D', ' ', 'F', 'l', 'a', 's', 'h', ' ',
        'D', 'i', 's', 'k', ' ',

        '1', '.', '0', ' '
      }